RSVPEEP(8) RSVPEEP(8)

NAME

rsvpeep − display multicast RSVP state

SYNOPSIS

rsvpeep [ −n ] [ −d address.port ] [ node_ID ] . ..

DESCRIPTION The RSVP daemon rsvpd is capable of multicasting UDP packets containing diagnostic information (a summary of its internal state) periodically and whenever the state changes. Rsvpeep is a command-line program to receive and display this state.

By default rsvpeep will display state from all nodes. However, if one or more node_ID parameters occur, rsvpeep will display only the state from the specified node(s). A node_ID is the first component of the DNS name of a node.

OPTIONS

−n Display all IP addresses in numeric (i.e., dotted-decimal) form, do not try to convert them to DNS names.

−d When it is configured to multicast state, rsvpd multicasts the state to address 224.0.1.19 and port 1427; by default, rsvpeep listens on this address and port. The −d option causes rsveep to instead listen on IP address address and UDP port port; they are separated by a period.

SEE ALSO

rsvpd, rstat

20 Sept 95 1