Date       ftp site
--------  ----------------------------------------------------------
06-9-98   ftp://ftp.xilinx.com/pub/swhelp/M1.4_alliance/spd_4kxl3_m14.zip

Combined xc4000xl speed file update and bitgen update for M1.4.

Solution 3971 - Updates xc4002xl speeds from Advanced to Preliminary

Solution 3970 - Fixes a timing problem with pullups in xc4002xl and a 
                wire segment in xc4085xl.

Solution 3703 - Fixes a bitstream problem with FCLKIOB in xc4002xl, 
                xc4005xl, and xc4010xl.

Solutions 3969 and 3727 - Fixes two seperate bitgen tiedown problems.

Solution 3666 - Fixes a bitstream problem with OMUX2.

Solution 4031 - Adds -08 speed grade to 4013xl, 4036xl and 4062xl.
 
The following installation instructions assume that there is already
a valid M1.4 environment set.
 
Use WinZip or equivalent utility to unzip  spd_4kxl3_m14.zip
into c:\xilinx or where ever the M1.4 tools are installed.

 

